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ABSTRAK

Perusahaan listrik saat ini masih mengandalkan tenaga manusia sebagai petugas pencatat data KWH meter yang harus datang setiap bulan. Sistem monitoring daya listrik selama ini masih dilakukan secara konvensional yaitu secara manual menggunakan alat pembaca meter oleh petugas PLN dengan mendatangi setiap rumah. Cara konvensional tersebut sangat mengurangi efisiensi waktu. Oleh karena itu, pada proyek akhir ini dibuat sistem monitoring daya listrik pada beberapa KWH meter secara wireless dengan sistem komunikasi serial multihop dan pencarian rute otomatis. Komunikasi serial multihop digunakan pada proses pengiriman data antar KWH meter dengan asumsi masing-masing KWH meter dapat saling berkomunikasi. Dengan menggunakan komunikasi serial multihop ini maka data pemakaian daya listrik pada KWH meter akan dikirimkan ke server secara point to point atau peer to peer setelah sebelumnya dilakukan proses RTS (Request To Send) dari pihak server untuk meminta data.  Metode multihop yang telah diterapkan mampu mendukung proses komunikasi data yang  dilakukan oleh server untuk mendapatkan data daya listrik pada beberapa KWH meter yang terletak cukup jauh dari jangkauan server. Proses komunikasi data pada monitoring daya listrik ini menggunakan baud rate 9600 dan telah menghasilkan tingkat keberhasilan penerimaan data yang optimal sebesar 95 %  bagi pihak server.Algoritma pencarian rute otomatis yang diterapkan dapat membantu kelancaran proses komunikasi data secara multihop pada monitoring daya listrik ini. Masing-masing kontroler pada KWH meter memiliki tabel rute pengiriman sehingga apabila ada salah satu KWH meter nonaktif yang mengakibatkan putusnya rute pengiriman maka kontroler pada KWH meter pembawa paket data terakhir secara otomatis mencari rute pengiriman baru.   
Kata kunci : KWH, Komunikasi, Wireless, Multihop, Rute Otomatis
ABSTRACT

The existing electrical company still relying on manpower as data logger officer KWH metre which must come each month. Electricity monitoring system till now still be done conventionally that is in manual applies equipment of reader metre by officer PLN by visiting every house. The conventional way hardly lessens time efficiency. Therefore, at project of this end made electricity monitoring system at some KWH metre in wireless with serial communications system of multihop and seeking of automatic route.Multihop serial communications applied at delivery process of data between KWH metre with assumption each KWH metre earns is each other communicate. By using serial communications of this multihop hence usage data of electricity at KWH metre will be sent to server in point to point or peer to peer after before all is done process RTS ( Request To Send) from the side of server to ask data.Multihop method which has been applied can support data communication process done by server to get electricity data at some KWH metre which is located far enough from server reach. Data communication process at this electricity monitoring applies baud rate 9600 bps and has yielded level of success of receiving acceptances of optimal data 95 % for the side of server.Seeking algorithm of automatic route applied able to assist fluency of data communication process in multihop at this electricity monitoring. Each controller at KWH metre has delivery route tables so that if there is one of KWH metre inactive resulting a  break delivery route hence controller at KWH metre last data package carrier automatically looks for new delivery route.

Keyword : KWH, Communication,Wireless, Multihop, Automatic Route
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